Some boards have a slightly older version of the factory\_loader which does not support auto detection of SPI and UART. In this case, legacy mode needs to be used by using --mode=legacy.

|  |
| --- |
| ./script/factory\_loader.py /dev/ttyUSB2 --mode=legacy helloworld\_config.json |