## Response Description & Payload

|  |  |  |
| --- | --- | --- |
| **Command** | **Response Description** | **Response Payload** |
| AT | OK/Error | NA |
| AT+WDIS | OK/Error | NA |
| AT+WSCAN | OK/Error | NA |
| AT+SOCSRV  Example: at+socsrv=0,1,1,9000 | OK | 0:CONNECT :0>>@:OK |
| AT+HCSTART  Example: at+hcstart=192.168.1.5,80 | OK | :CONNECT:0>>@:OK |

Table 4: AT Commands – Response description and payload

## Running the Application

For more details regarding running the AT Commands application, refer: Run the Application in the QSG.