# Prerequisites

1. Talaria TWO Evaluation Board
2. Serial Cable (USB to Micro-USB)
3. Windows/Linux PC
4. Wi-Fi Access Point/Network
5. Minicom/Tera Term VT Utility installed on PC

AT enables the host micro-controller to interface with the Talaria TWO EVB using AT commands over UART (currently supported), SPI or SDIO port.

**Note**: The EVB is shipped with pre-loaded AT application firmware. If there is a need to reinstall the firmware or install a higher version of the firmware, follow the instructions provided in section: *Download the Necessary Packages*. Otherwise, skip to section: *Configure the Serial Port* with pre-loaded firmware.

## Download the Necessary Packages

### Download the Evaluation and Software Development Package (SDK)

*Check with your InnoPhase IoT support team to obtain the latest version of the FreeRTOS evaluation and SDK packages*.

Download the SDK zip file and extract the same.