## Configure the Serial Port

This section provides Serial Host interface configuration to send serial data (AT commands) to Talaria TWO. The host can be interfaced with Talaria TWO over UART/SPI. The default UART configuration is as follows:

1. Baud Rate: 115200bps
2. Data: 8 bits
3. Parity: None
4. Stop bits: 1 bit
5. Flow Control: None

Using Teraterm, select USB Port #5 and baudrate 9600 since the firmware is configured with baudrate=9600.

Graphical user interface, application

Description automatically generated

Figure 4: Tera Term Setup