This section describes the different AT commands use cases with details on the prerequisites, sequence of operation and expected output.

**Note**: The EVB is shipped with pre-loaded AT application firmware. If there is a need to reinstall the firmware or install a higher version of the firmware, follow the instructions provided in section: *Download the Necessary Packages* of the AT Commands Quick Start Guide:

# Set-up & Usage

## Pre-set-up on Talaria TWO

## Programming the Application

# UseCases

## Wireless Operations

### Station Mode

### Power Management

### BLE Peripheral

### BLE IO Capabilities

## Network Protocol

### Static IP Configuration

### Ping & Reset Functionality

## Application Protocol and Data Transfer

### TCP Server

### TCP Client

### UDP Server

### UDP Client

### HTTP Client

### MQTT Client

### Secure MQTT

### DNS Lookup – Get Host IP by Name

### Service Discovery using mDNS

### Get Time from NTP Server

## Advances Services

### BLE Provisioning

### Secure BLE Provisioning by Passkey Method

### Secure BLE Provisioning by Just Works Method

### FOTA

## Miscellaneous

### Echo Enable/Disable