Talaria TWO (INP1014) module on the INP3201 board can be programmed using the SWD mode. Ensure the following while programming the module:

1. Programing Talaria TWO (INP1014) without powering up INP3201: Talaria TWO module can be programmed using the SWD connector J6 on the module. Power to the Talaria TWO module can be supplied through the SWD connector from the INP3000 board rev 5.0.:



Figure 7: INP3201 J6 SWD connector for Talaria TWO

A circuit board with wires attached to it

Description automatically generated

Figure 8: Talaria TWO SWD programming

**Note**: If the INP3201 is already powered through Type C USB cable, ensure to remove the 3.3V power Jumper J9 on the programmer board INP3000 as indicated in Figure 8.