## Testing for Basic Operations

There are three application init scripts in /system/init folder:

1. app\_init.sh: Basic functionality (using connection manager commands)
2. app\_init\_t2.sh: Talaria TWO used for power management (copy this script to app\_init.sh)
3. app\_init\_mcu.sh: STM32 MCU used for power management (copy this script to app\_init.sh)

When T31zx booting is completed, the init script loads the sdio-wlan.ko driver module and runs the tunadapter application as an initial step to use the Talaria TWO Dual-Stack commands.

For more details on the tunadapter, refer: UG\_Dual\_Stack.pdf (*talaria\_two\_dual\_stack\_vx.y\host\INP3201\doc*).