## Boot Arguments

Talaria TWO’s software allows the user to pass boot time arguments which might be useful during the execution of the software. Users can pass boot time arguments to configure the firmware. In the current use case, the following boot arguments are passed:

|  |
| --- |
| BLE5\_adv\_mode=0,BLE5\_adv\_sec\_phy=0 |

A screenshot of a computer

Description automatically generated

Figure 24: Passing Boot Arguments