## Resetting the EVB-A in BL Mode

To reset the EVB-A in Boot Loader mode, click on Reset in BL Mode as shown in Figure 25.

A screenshot of a computer

Description automatically generated

Figure 25: Reset in BL mode

When the EVB-A is reset in the Boot Loader mode, though no changes are observed in the console for this command, the board is reset.