## Installation Instructions for libusbK Driver

Download the free software Zadig, available here: - [**https://zadig.akeo.ie/**](https://zadig.akeo.ie/)**.** Connect your Windows PC or Laptop to the evaluation board using the provided USB cable. Now, open Zadig and click on Options. Select List All Devices and deselect Ignore Hubs or Composite Parents as shown in Figure 8.

A screenshot of a computer

Description automatically generated

Figure 8: Listing devices in Zadig

To establish communication with Talaria TWO module via the FTDI device on the InnoPhase Evaluation Board, the Talaria TWO USB driver must be libusbK. In case the current driver is not libusbK, use the drop-down menu to select libusbK and click on Replace Driver which will update the drivers to libusbK.

Graphical user interface, text, application, Word

Description automatically generated

Figure 9: Updating Talaria TWO USB driver to libusbK