## Echo Enable/Disable

### Description

This use case is used to demonstrate echo enable and disable.

### Prerequisites

None.

### AT Command Sequence

|  |  |
| --- | --- |
| **AT Command** | **Description** |
| *at* | Check communication state |
| *at+echo* | Enable/Disable the Command Echo Feature |

Table 30: Echo enable/disable - AT Commands

### Procedure

**Step 1**: Execute the followings commands on Talaria TWO:

|  |
| --- |
| at  at+echo=1  at  at+echo=0 |

### Serial Log

Graphical user interface, text, application

Description automatically generated

Figure 123: Echo enable/disable - Serial log