The MCU STM32L010F4P6 on INP3201 can be programmed using the connector J3:



Figure 9: Programming STM32 MCU

The bin file for STM32L010F4P6 is provided as part of the software package and STlink can be used to program the MCU.

For more details, refer: MUC\_Firmware\_Flashing